These programs can be selected by SW switch OR set as default with dipswitches

01 OS8 disk server load 40/41  
02 MI8-EA paper tape  
03 MI8-EC TC08 dec tape  
04 MI8-ED RK8  
05 MI8-EE Typeset  
06 MI8-EF Edu sys low  
07 MI8-EG Edu sys high

10 RX8 bootloader  
11 RX28  
12 RIM loader   
13 BIN LOADER  
14 MI8-EH TD8-E  
15 Wipe core field 0

The next can only be loaded by toggling the SW switch or pushbutton on the PCB only.

20 group 1 microinstructions  
21 group 1 microinstructions  
22 Operate instructions  
23 ISZ instructions  
24 JMS instruction  
25 JMP instruction  
26 AC increment  
27 checker board runs endless MD alters between 0000 and 7777

30 checker board runs endless MD alters between 5252 and 2525  
31 print character in switch register  
32 console print test  
33 Echo test for one terminal at 03/04  
34 echo 1-4 terminals